#...............................................................................
#
#  I2C/SPI Tap session plugin
#

[plugin]

name        = "I2C/SPI Tap"
description = "Monitor I2C/SPI communication via an I2C/SPI Tap device from Tibbo"
id          = i2c-spi-tap
group       = serial
monitor     = true
log-guid    = 39ee6b0f-a65e-4e8a-b252-6fa28d8e3327  # i2c-spi tap
log-guid    = b26c1b57-16c7-48a5-bbb9-05ea1ada5368  # fpga uploader
icon        = images/sniffer.png
small-icon  = images/sniffer-16x16.png

session-class = I2cSpiTapSession

[required-capabilities]

com.ioninja.io.i2c-spi-tap
org.jancy.io.file

[scripts]

Decoder.jnc
I2cSpiTapSession.jnc
I2cDecoder.jnc
SpiDecoder.jnc
